**Standard Coordination Phantoms Concept:**

* **Network voltage : 400V**
* **Control voltage : 230V**
* **Combination according to standard steps file on server**
* **Phantom include the following:**
* Complete combination:

Capacitor step , Fuse , Fuse base , Contactor(if needed) & Splitter

* **Phantom not include the following:**
* Installation accessories ( long terminal shield , bare cable , ….)
* Any control components ( Varlogic , fans , handle for fuse , …)