**Standard Coordination Phantoms Concept:**

* **Network voltage : 415V**
* **Control voltage : 230V or 220V**
* **Combination installed in MF cubicle**
* **Coordination Selection & Breaking capacity:**

Up to 5.5KW : Combination is with GV2P & withstand 85KA

Higher than 5.5KW : Combination is with NSX – H & withstand 70KA

* **Phantom include the following:**
* Complete combination : C.B , Contactor & Overload
* Standard auxiliaries (OF & SDE & Black extended rotary handle)
* Overload base if needed according to catalogue
* **Phantom not include the following:**
* Installation accessories ( long terminal shield , bare cable , ….)
* Any control components ( Lamps , relays , selectors , ….)