**Standard Coordination Phantoms Concept:**

* **Network voltage : 415V**
* **Control voltage : 230V**
* **Combination installed in MF cubicle**
* **Coordination Selection & Breaking capacity:**

Up to 37KW @ 30® : Combination is with NS80H & withstand 70KA

Higher 37KW @ 30® : Combination is with NSX – H & withstand 70KA

* **Phantom include the following:**
* Complete combination:

C.B , Contactor , Soft Starter , Fuse, Fuse accessories , Fans ( if needed )

* Standard auxiliaries (OF & SDE & Black extended rotary handle)
* **Phantom not include the following:**
* Installation accessories ( long terminal shield , bare cable , ….)
* Any control components ( Lamps , relays , selectors , ….)